[bookmark: _Hlk496791321]
[image: ]

Please Note:
This template is intended for educational purposes only, without any express or implied warranty of any kind, including warranties of accuracy, completeness, or fitness for any particular purpose.  You agree that your use of the template is without any recourse whatsoever to PG&E, SCE, SDG&E, or their affiliates. The template is a draft, and anyone using this document should seek the advice of an attorney to develop appropriate ordinance language to meet its jurisdiction’s specific needs, as state and local laws may differ.

This document is the product of a collaborative effort between Peninsula Clean Energy, Silicon Valley Clean Energy, and the Local Energy Codes team. 

Please contact the Codes and Standards Local Energy Codes Team at info@LocalEnergyCodes.com for additional information.


This program is funded by California utility customers and administered by Pacific Gas and Electric Company, San Diego Gas & Electric Company (SDG&E®), and Southern California Edison Company under the auspices of the California Public Utilities Commission and in support of the California Energy Commission.



REACH CODE IMPLEMENTATION RESOURCES TEMPLATE
2025 SINGLE FAMILY ADDITIONS and ALTERATIONS CHECKLIST
Version 1.0, January 2026

This template is provided to assist local jurisdictions with the implementation of adopted reach codes. It is not intended to provide guidance on the development of a reach code ordinance. Anyone developing a reach code ordinance should seek the advice of an attorney to develop appropriate ordinance language to meet its jurisdiction’s specific needs, as state and local laws may differ. This template is intended for educational purposes only, without any express or implied warranty of any kind, including warranties of accuracy, completeness, or fitness for any particular purpose. You agree that your use of the template is without any recourse whatsoever to the developers of this document. 

This document is intended as a compliance tool for typical 2025 local reach codes. 
Modify it as needed to suit local requirements (especially blue italicized text). 

Scope
This checklist includes requirements for certain additions and alterations that align with the following model reach codes:
· Flexible Compliance Pathway (FlexPath)
· Electric Readiness
· Electric Service Panel Upgrade
· Cool Roofs
A separate form is available for air conditioner replacements/additions.

Instructions
· Make modifications following instructions and options in blue text. DELETE ALL BLUE TEXT AND COMMENTS BEFORE PUBLISHING.
· Delete sections that do not apply, renumber sections as needed and edit requirements to align with local ordinance.
· Check all numbering and internal references after editing.
LOCAL BUILDING DECARBONIZATION CHECKLIST 
SINGLE FAMILY ADDITIONS AND ALTERATIONS CHECKLIST
LOCAL LOGO

· Delete the cover page and this page.


When to Use this Form
This form is required for all additions and alterations to single family homes, duplexes and townhomes. If your project is limited to replacing or adding an air conditioner only, [Option A: “use the AC Replacement Checklist.” Option B: “you may either use the AC Replacement Checklist or satisfy the FlexPath requirements using this form.”] 	Comment by Author: CUSTOMIZATION: Modify this text to align with the adopted FlexPath and AC to Heat Pump ordinances as appropriate.

[bookmark: _Hlk497744841][bookmark: _Hlk497742754]These building standards have been established to ensure that construction in [jurisdiction] is healthier for occupants, has limited impact on the environment, reduces demand for energy, and results in cost savings from building operation over the life of the building. This checklist is intended to help applicants understand 
the process and specific local requirements that apply to their project.

For more information, please visit [jurisdiction website or other resource]


PROJECT PROCESS

1. Project Design

It is important for project owners, architects, engineers, and designers to understand the applicable state and local building requirements prior to project design. Early consideration of these standards allows for design of buildings and systems that are compliant, energy efficient, and cost effective, and minimizes back and forth when applying for the project permit.


2. Planning Application (If required)

If your project is subject to a zoning variance or planning review, be prepared to identify in your planning application what compliance methods you’ve selected and how you plan to meet the requirements. If you anticipate difficulties meeting the requirements, these concerns and any requests for exemptions should be identified in your planning application.


3. Initial Building Permit Submittal

Include the following on your plans as part of your initial application for a building permit:
· Completed Local Building Decarbonization Checklist
· Title 24 Part 6 documentation demonstrating compliance with all State requirements
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Modify this document to suit local requirements (especially blue italicized text). 
DELETE ALL BLUE TEXT AND COMMENTS BEFORE PUBLISHING
Version 1.0, January 2026
This form is required for all additions and alterations to 
single family homes, duplexes and townhomes


PROJECT ADDRESS:______________________________________________________________

APN:___________________ APPLICANT NAME:________________________________________

Climate Zone: _______ 
(To find the climate zone, visit the California Energy Commission Climate Zone Tool Finder.)	Comment by Author: CUSTOMIZATION: Delete if only one climate zone.

Project Scope and Requirements. Check all that apply.
A. Table 1: FlexPath  
	Check
	Project Scope
	Checklist Instructions

	☐	Project scope includes: [Description of Covered Project] (check all that apply)
☐ Addition or alteration that impacts floor area equal to or greater than XXX square feet, OR
☐ YYYY, OR
☐ ZZZZ 
	Complete Section 
3 and Section 7

	☐	FlexPath Express Compliance (All must be checked to meet Express Compliance requirements):
☐  Project or home includes a heat pump space heater or heat pump water heater, AND
☐  Project or home includes all high efficacy screw-in light bulbs (e.g., LEDs), AND
☐  Project does not trigger electric readiness requirements
	Complete Section 
3A and Section 7

	☐	Project is limited to adding or replacing an air conditioner (and associated measures)	Comment by Author: CUSTOMIZATION: Include this row only if your FlexPath ordinance includes AC replacements/additions in the definition of a Covered Project.  This option provides flexibility for AC changeouts selecting the AC Pathway (not hp) to install other measures that achieve equivalent energy savings.
☐  Air conditioner will be replaced with heat pump
☐  Air conditioner will be replaced with like-for-like equipment (air conditioner)
	HP: Skip to Section 7
AC: Complete Section 3 and Section 7 or complete AC Replacement Checklist	Comment by Author: CUSTOMIZATION: Include this if you have a separate AC replacement ordinance.

	☐	None of the above
	Skip to Section 7



B. Table 2: Electric Readiness
	Check
	Project Scope
	Checklist Instructions

	☐	Project scope includes (check all that apply):
☐ Circuits added or altered within three feet of a gas water heater, range, stovetop, oven, or clothes dryer, OR
☐ Framing altered within 3 feet of a gas water heater, OR
☐ A gas line(s) extended to an outdoor appliance
	Complete Section 
4 and Section 7

	☐	Main electrical service panel is being upgraded
	Complete Section 
5 and Section 7

	☐	None of the above
	Skip to Section 7



C. Table 3: Cool Roof
	Check
	Project Scope
	Checklist Instructions

	☐	More than 50% of roof being replaced (including adding a new surface layer on top of the existing exterior surface)
	Complete Section 
6 and Section 7

	☐	None of the above
	Skip to Section 7



These requirements are specified in the following Sections of [Jurisdiction’s] Municipal Code: [specify local code sections]
· FlexPath
· Electric Readiness
· Cool Roof
Exemptions. 	Comment by Author: CUSTOMIZATION: Edit list as needed.
If any apply, check and skip to Section 7.
☐	The project is solely related to any of the following: a repair, as defined by Title 24 Part 2 Section 202; medically necessary improvements; seismic safety improvements; safety improvement to remove a known hazard; roofing-only projects; fenestration-only projects; or Emergency Housing pursuant to Appendix P of the California Building Code.	Comment by Author: CUSTOMIZATION: Delete if cool roofs are part of the reach code.
☐	The project is solely related to a new attached accessory dwelling unit or junior accessory dwelling unit with expansion of not more than 150 square feet to accommodate ingress and egress.
☐	This project is a mobile home, manufactured home or factory-built home.
☐	 The project does not meet the requirements for an exemption as listed above, but is eligible for a different exception. Identify the exception number and provide a short description below.  Contact the [City/County of XXXX] Building Department to review the project details and confirm the project eligibility for the exception.  



[bookmark: _Flexible_Compliance_Option]Flexible Compliance Option (FlexPath). 
This section is required for projects that [insert or refer to definition of covered project].
A. 	Express Compliance. 	Comment by Author: CUSTOMIZATION: This section is optional. It is intended to encourage applicants to choose an electrification pathway. It is not intended to be comprehensive.
If all boxes below can be checked, skip to Section 7.	Comment by Author: CUSTOMIZATION: Edit list to include the most basic requirements necessary for compliance.
The project includes, or the home already has, a heat pump space heater or a heat pump water heater
All screw-in light bulbs are high-efficiency (e.g., LEDs)
The project does not include any activities that trigger electric readiness requirements in Section 4 or electrical service panel upgrade requirements in Section 5.

B.	Flexible Compliance.
1. Target Score
Complete Table 4. First, select the project vintage to identify the Target Score. Complete Table 5 after selecting measures from Table 6 that meet or exceed the Target Score.

Table 4: Project Vintage and Target Score – Climate Zone [XX]	Comment by Author: CUSTOMIZATION: Use values from the ordinance.
	
	Pre-1978
Vintage
	1978-1991
Vintage
	1992-2010
Vintage

	Select project vintage ®
	☐	☐	☐
	Target score by vintage ®
	X
	Y
	Z



Table 5: Target Score and Total Points Claimed – Climate Zone [XX]
	Line
	Compliance With Target Score
	Points

	A
	Enter Total Points Claimed from Table 6 ®
	

	B
	Enter the Target Score for project vintage from Table 4 ®
	

	C
	Subtract Line B from Line A – Result must be zero or greater ®
	



2. Measure Menu
1. Complete Table 6 by selecting a measure or a combination of measures that adds up to at least the Target Score for the project vintage in Table 4.  
2. In the far-right column of Table 6, enter the total points associated with the project vintage for each measure newly or previously installed. For measures previously installed, submit supporting documentation demonstrating compliance with the requirement.
3. Complete Table 5 to document that project meets the Target Score. Enter the sum of the Total Points Claimed from Table 6.
4. Refer to Table 9: Measure Specifications for specific measure requirements.

Table 6: Energy and Electrification Menu of Measures by Vintage	Comment by Author: CUSTOMIZATION: Use the Cost Effectiveness Explorer to identify the point values for each measure. Delete unused measures and number ID to match specification table. 
	ID
	
	Pre- 1978
Vintage
	1978-1991
Vintage
	1992-2010
Vintage
	Points Claimed

	
	Select Project Vintage 
	☐	☐	☐	

	E1
	Lighting Measures
	Mandatory
	Mandatory
	Mandatory
	

	E2
	Water Heating Package
	[x]
	[x]
	[x]
	

	E3
	Air Sealing 
	[x]
	[x]
	[x]
	

	E4.A
	R-38 Attic Insulation
	[x]
	[x]
	[x]
	

	E4.B
	R-49 Attic Insulation
	[x]
	[x]
	[x]
	

	E5
	Duct Sealing
	[x]
	[x]
	[x]
	

	E6.A
	New Ducts, R-6 Insulation + Duct Sealing
	[x]
	[x]
	[x]
	

	E6.B
	New Ducts, R-8 Insulation + Duct Sealing
	[x]
	[x]
	[x]
	

	E7
	Windows
	[x]
	[x]
	[x]
	

	E8
	Wall Insulation
	[x]
	[x]
	[x]
	

	E9.A
	R-19 Raised floor insulation
	[x]
	[x]
	[x]
	

	E9.B
	R-30 Raised floor insulation
	[x]
	[x]
	[x]
	

	E10
	Cool Roof
	[x]
	[x]
	[x]
	

	E11
	Radiant Barrier Under Roof
	[x]
	[x]
	[x]
	

	FS1
	Heat Pump Water Heater Replacing Gas
	[x]
	[x]
	[x]
	

	FS2
	High Eff. Heat Pump Water Heater Replacing Gas
	[x]
	[x]
	[x]
	

	FS3
	Heat Pump Water Heater Replacing Electric
	[x]
	[x]
	[x]
	

	FS4
	High Eff. Heat Pump Water Heater Replacing Electric
	[x]
	[x]
	[x]
	

	FS5
	Heat Pump Space Conditioning System
	[x]
	[x]
	[x]
	

	FS6
	High Eff. Heat Pump Space Conditioning System
	[x]
	[x]
	[x]
	

	FS7
	Dual Fuel Heat Pump Space Conditioning System
	[x]
	[x]
	[x]
	

	FS8
	Heat Pump Clothes Dryer
	[x]
	[x]
	[x]
	

	FS9
	Induction Cooktop
	[x]
	[x]
	[x]
	

	PV
	Solar PV + Electric Readiness
	[x]
	[x]
	[x]
	

	Total Points Claimed: (enter here and in Table 5, line A) 
	





[bookmark: _Electric_Readiness]Electric Readiness
Check the boxes if the project includes any of the electric readiness measures listed in Table 7.
Table 7: Electric Readiness
	Check 
	Scope
	Requirement

	☐	Water Heater: Circuit added or altered within 3 feet of an existing gas water heater or within 10 feet of a designated location of a future water heater
	Electrical readiness* at 240V/30A


	☐	Water Heater: Wall framing removed or replaced adjacent to water heater
	Reserve space for heat pump water heater (minimum 2.5 feet by 2.5 feet wide and 7 feet tall) and install a condensate drain

	☐	Range/Stovetop/Over: Kitchen circuit added or altered within 3 feet of a gas appliance
	Electrical readiness* at 240V/50A

	☐	Clothes Dryer: Laundry area circuit added or altered within 3 feet of a gas appliance
	Electrical readiness* at 240V/30A

	☐	Outdoor Gas Appliance: Gas line extended to outdoor appliance (other than an emergency power generator)
	Install conduit or a circuit designed to serve a future electric appliance(s) with the same function, including the appropriate voltage, phase, minimum amperage, and an electrical receptacle or junction box within five feet of the appliance



*	Electric readiness: Within 3 feet of appliance install either a) a 120V/20-amp circuit, with conductors with capacity to support conversion to 3 conductor (plus ground) 240V circuit at the specified amperage or b) a raceway (conduit or sheathed cable) between main panel and an enclosure at the appliance capable of supporting a 3 conductor (plus ground) 240V circuit at the specified amperage.




[bookmark: _Electrical_Service_Panel]Electrical Service Panel Upgrade
This section must be completed for all projects involving an upgrade of the main electrical service panel.
Calculations are required in accordance with California Electrical Code Article 220.83 determining that future loads will exceed the capacity of the current electrical power infrastructure and calculations, and, where historical data are available, in accordance with California Electrical Code Article 220.87 determining that future loads exceed the capacity of the current electrical service infrastructure.
The calculations must include one of the following (check at least one):
☐	At least one power management or circuit controlling device, serving electric-only appliances such as: water heater; clothes dryer; range; Level 2 EV charging receptacle; or Low Power Level 2 EV charging receptacle.
Specify the appliance: __________________
☐	At least one of the following electric-only appliances operating on 120V: water heater; clothes dryer; range.
Specify the appliance: __________________
☐	Circuit control between whole home load and Level 2 EV Charging Receptacle or Low Power Level 2 EV Charging Receptacle

Calculations are provided as part of the plan submittals:
California Electrical Code Article 220.83
California Electrical Code Article 220.87
Data are not available to support Article 220.87 calculations
State reason: ____________________________________________
Exemption
The panel upgrade is for required electrical improvements supporting loads other than water heaters, dryers, ranges/stovetops/ovens, or electric vehicle chargers.
Specify end use that requires panel upgrade: __________________



[bookmark: _Roof_Replacements]Roof Replacements
Complete this section if replacing more than 50% of the existing roof area. Roofing products must be rated by the Cool Roof Rating Council (CRRC). 

Table 8: Roof Replacements 
	Check 
	Scope
	Requirement
	Installed Values

	☐	Roofing: Replacement of 50% or more of roof
	Install a cool roof with an aged solar reflectance equal to or greater than:
· Steep-sloped (greater than 2:12): 0.25
· Low-sloped (2:12 or less): 0.65 
	
Steep-sloped: ______        
Low-sloped:    ______



[bookmark: _Hlk216767892]
[bookmark: _Project_Verification]Project Verification
This form has been completed by _________________(name) of ___________________(company), the qualified [specify credentials based on local practice, e.g., architect, engineer, project manager] individual for the above listed project who verifies that it accurately represents the project plans. [modify based on local verification requirements]



________________________________			______________
Signature								Date
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Table 9: FlexPath Measure Specifications
	ID
	Energy Efficiency Measures

	E1
	Lighting Measures – Install lighting with an efficiency of 45 lumens per watt or greater in all interior and exterior screw-in fixtures. Install photocell, occupancy sensor or energy management system controls that meet the requirements of 150.0(k)3 in all outdoor lighting permanently mounted to a residential building or to other buildings on the same lot.

	E2
	Water Heating Package: Insulate all accessible hot water pipes with pipe insulation a minimum of ¾ inch thick. This includes insulating the supply pipe leaving the water heater, piping to faucets underneath sinks, and accessible pipes in attic spaces or crawlspaces. Upgrade fittings in sinks and showers to meet current California Green Building Standards Code (Title 24, Part 11) Section 4.303 water efficiency requirements.
Exception: Upgraded fixtures are not required if existing fixtures have rated or measured flow rates of no more than ten percent greater than 2025 California Green Building Standards Code (Title 24, Part 11) Section 4.303 water efficiency requirements.

	E3
	Air Sealing: Seal all accessible cracks, holes, and gaps in the building envelope at walls, floors, and ceilings. Pay special attention to penetrations including plumbing, electrical, and mechanical vents, recessed can light luminaires, and windows. Weather-strip doors if not already present. Verification shall be conducted following a prescriptive checklist that outlines which building aspects need to be addressed by the permit applicant and verified by an inspector. Compliance can also be demonstrated with blower door testing conducted by a certified ECC Rater no more than three years prior to the permit application date that either: a) shows at least a 30 percent reduction from pre-retrofit conditions; or b) shows that the number of air changes per hour at 50 Pascals pressure difference (ACH50) does not exceed ten for Pre-1978 vintage buildings, seven for 1978 to 1991 vintage buildings and five for 1992-2010 vintage buildings. If combustion appliances are located within the pressure boundary of the building, conduct a combustion safety test by a certified ECC Rater or a professional certified by the Building Performance Institute, in accordance with the BPI Technical Standards for the Building Analyst Professional.

	E4.A
	R-38 Attic Insulation: Attic insulation shall be installed to achieve a weighted assembly U-factor of 0.025 or insulation installed at the ceiling level shall have a thermal resistance of R-38 or greater for the insulation alone. Recessed downlight luminaires in the ceiling shall be covered with insulation to the same depth as the rest of the ceiling. Luminaires not rated for insulation contact must be replaced or fitted with a fire-proof cover that allows for insulation to be installed directly over the cover. 
Exception: In buildings where existing R-30 is present and existing recessed downlight luminaires are not rated for insulation contact, insulation is not required to be installed over the luminaires.

	E4.B
	R-49 Attic Insulation: Attic insulation shall be installed to achieve a weighted assembly U-factor of 0.020 or insulation installed at the ceiling level shall have a thermal resistance of R-49 or greater for the insulation alone. Recessed downlight luminaires in the ceiling shall be covered with insulation to the same depth as the rest of the ceiling. Luminaires not rated for insulation contact must be replaced or fitted with a fire-proof cover that allows for insulation to be installed directly over the cover. Exception: In buildings where existing R-30 is present and existing recessed downlight luminaires are not rated for insulation contact, insulation is not required to be installed over the luminaires.

	E5
	Duct Sealing: Air seal all space conditioning ductwork to meet the requirements of the 2025 Title 24, Part 6, Section 150.2(b)1E.  The duct system must be tested by a ECC Rater no more than three years prior to the Covered Single Family Project permit application date to verify the duct sealing and confirm that the requirements have been met.  This measure may not be combined with the New Ducts and Duct Sealing measure in this Table.
Exception: Buildings without ductwork or where the ducts are in conditioned space.

	E6A
	[Climate Zones 3, 5, 6, 7 only (R-8 required prescriptively elsewhere)] New Ducts, R-6 insulation + Duct Sealing: Replace existing space conditioning ductwork with new R-6 ducts that meet the requirements of 2025 Title 24, Part 6, Section 150.0(m)11. This measure may not be combined with the Duct Sealing measure in this Table.  To qualify, a preexisting measure must have been installed no more than three years before the Covered Single Family Project permit application date.

	E6B  Alternate
	New Ducts, R-8 insulation + Duct Sealing: Replace existing space conditioning ductwork with new R-8 ducts that meet the requirements of 2025 Title 24 Section 150.0(m)11. This measure may not be combined with the Duct Sealing measure in this Table.  To qualify, a preexisting measure must have been installed no more than three years before the Covered Single Family Project permit application date.

	E7
	Windows: Replace at least 50% of existing windows with high performance windows with an area-weighted average U-factor no greater than 0.27.

	E8
	R-15 Wall Insulation: Install wall insulation in all exterior walls to achieve a weighted U-factor of 0.095 or install wall insulation in all exterior wall cavities that shall result in an installed thermal resistance of R-15 or greater for the insulation alone.

	E9.A
	R-19 Floor Insulation: Raised-floors shall be insulated such that the floor assembly has an assembly U-factor equal to or less than U-0.037 or shall be insulated between wood framing with insulation having an R-value equal to or greater than R-19.

	E9.B
	R-30 Floor Insulation: Raised-floors shall be insulated such that the floor assembly has an assembly U-factor equal to or less than U-0.028 or shall be insulated between wood framing with insulation having an R-value equal to or greater than R-30.

	E10
	[Climate Zones 6-15 only. This item can be required as a mandatory measure for a reroofing project. See Flex Path Decision Guide for details] Cool Roof : Install a cool roof on at least 50% of the roof area. For steep-sloped roofs (ratio of rise to run greater than 2:12) install a roofing product rated by the Cool Roof Rating Council to have an aged solar reflectance equal to or greater than 0.25 and a thermal emittance equal to or greater than 0.75.

	E11
	Radiant Barrier: A radiant barrier that meets the requirements of Section 150.1(c)2 shall be installed under at least 50% of the roof surface.

	ID
	Fuel Substitution and Solar PV Measures

	FS1
	Heat Pump Water Heater (HPWH) Replacing Gas: Replace existing natural gas water heater with a heat pump water heater that meets the requirements of Sections 110.3 and 150.2(b)1Hiiib.

	FS2
	High Efficiency Heat Pump Water Heater (HPWH) Replacing Gas: Replace existing natural gas water heater with heat pump water heater with a Northwest Energy Efficiency Alliance (NEEA) Tier 3 or higher rating that also meets the requirements of Sections 110.3 and 150.2(b)1Hiiic.

	FS3
	Heat Pump Water Heater (HPWH) Replacing Electric: Replace existing electric resistance water heater with a heat pump water heater that meets the requirements of Sections 110.3 and 150.2(b)1Hiiib.

	FS4
	High Efficiency Heat Pump Water Heater (HPWH) Replacing Electric: Replace existing electric resistance water heater with heat pump water heater with a Northwest Energy Efficiency Alliance (NEEA) Tier 3 or higher rating that also meets the requirements of Sections 110.3, and 150.2(b)1Hiiic.

	FS5
	Heat Pump Space Conditioning System: Replace all existing gas and electric resistance primary space heating systems with a heat pump system that meets the requirements of Sections 110.2, 150.2(b)1.C, 150.2(b)1E, 150.2(b)1F, and 150.2(b)1G.

	FS6
	High Efficiency Heat Pump Space Conditioning System: Replace all existing gas and electric resistance primary space heating systems with an electric-only heat pump system that meets the requirements of Sections 110.2 and 150.2(b)1.C, 150.2(b)1E, 150.2(b)1F, and 150.2(b)1G and one of the following:
A. A ducted heat pump system with a SEER2 rating of 16.5 or greater, an EER2 rating of 12.48 or greater and an HSPF2 rating of 9.5 or greater; or
B. A ductless mini-split heat pump system with a SEER2 rating of 16.0 or greater, an EER2 rating of 12.0 or greater and an HSPF2 rating of 9.0 or greater

	FS7
	Dual Fuel Heat Pump Space Conditioning System: Install a heat pump space conditioning system that meets the requirements of Sections 110.2 and 150.2(b)1.C, 150.2(b)1E, 150.2(b)1F, and 150.2(b)1G and either: 
A. Replaces all existing gas and electric resistance primary heating systems with a hybrid gas and electric heat pump system, or
B. Is an electric-heat pump system in tandem with a gas furnace and controls to use the gas furnace for backup heat only.

	FS8
	Heat Pump Clothes Dryer: Replace existing electric resistance or gas clothes dryer with heat pump dryer with no resistance element and cap gas line.

	FS9
	Induction Cooktop: Replace all existing gas and electric resistance stove tops with induction stove top and cap the gas line.

	PV.A
	Solar PV: Install a solar PV system that meets the requirements of Section 150.1(c)14.

	PV.B Alternate 
	Solar PV + Electric Readiness: Install a solar PV system that meets the requirements of Section 150.1(c)14. In addition, for existing PV systems that had been installed prior to the application date of the current project, meet at least two [or more] of the electric readiness requirements in Section 150.0(x)1-6, regardless of whether they are otherwise required and regardless of the exceptions to Section 150.0(x).	Comment by Author: CUSTOMIZATION: If measures have been added or removed, edit reference to which subsections of Section 150.0(x) apply.
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